

**Video**

**Training**

**Document**

Contents

[I. Setup Github account and push data: 3](#_Toc131436853)

[II. Introduction of Video 6](#_Toc131436854)

[III. Display Resolution 8](#_Toc131436855)

[ Overscan and underscan- 8](#_Toc131436856)

[ Interlaced and progressive scan- 8](#_Toc131436857)

[ What is a Pixel ? 9](#_Toc131436858)

[ What is the Aspect Ratio? 10](#_Toc131436859)

[ What is the meaning of P and I in Resolution? 10](#_Toc131436860)

[ Different Types of Video Resolutions 11](#_Toc131436861)

[ Video Resolution Chart 11](#_Toc131436862)

[ Standard Definition 12](#_Toc131436863)

[ High Definition 12](#_Toc131436864)

[ Full HD 12](#_Toc131436865)

[ 2K Resolution 13](#_Toc131436866)

[ Ultra High Definition 13](#_Toc131436867)


[ 8K Resolution 13](#_Toc131436868)

[Formats of video files- 13](#_Toc131436869)


# Setup Github account and push data:

1. Create github account or sign in with your existing github account.

(website: <https://github.com/> )




1. By using your mail-id you can sign in or sign up on github.




3. Fill the details and create password and solve the puzzle.


1. At the end, click on create account and your github account will be created.
2. After login to your account, create one repository as shown.



1. **And create new repo**
2. **Open repo**
3. Enter your repo name and select privacy as public or private as per requirement. And select create repository.



1. By using SSH url will be used for push or pull data from github account.



1. Configuration and setup-

You have to add a remote repo url to your local git config by using command-

**git remote add <remote\_name > <remote\_repo\_url>**

This command will map remote repository at to a ref in your local repo under.

After mapping you can push local branches to it.

**git push -u <remote\_name> <local\_branch\_name>**

1. While push any data username and password, have to enter. This password will be a token number and can be generate by following link-

<https://docs.github.com/en/authentication/keeping-your-account-and-data-secure/creating-a-personal-access-token>

# Introduction of Video

A sequence of images processed electronically into an analog or digital format and displayed on a screen with sufficient rapidity as to create the illusion of motion and continuity.

A video is the art of integrating audio and visual elements into one form of multimedia, providing the audience with an image that is recorded electronically by a video camera and displayed on a television or device screen. Videos can be used for education, entertainment, or other purposes, which use pictures, graphics, or text.

Technology that involves the recording and playing back of moving pictures and sound: The next generation of interactive video technology will blend the viewer's image directly into the action on screen.

Light waves of object passes through lens, that light converted into electrical signals using Charge Coupled Device (CCD). In cameras three CCD use for three different hue (R, G, and B).

Video follow three standards:

1. Luminance: Brightness of pixel.
2. Chrominance: Color information
3. Synchronization: Series of electronic pulses that control by time of each frame of video.

* Video is categorized in two types-

1. Analog Video
2. Digital Video

The analog process encodes video and audio in complete frames (modulation), with the receiving device interpreting and translating the signal into video and audio on a monitor (de-modulation). This process can introduce a progressive loss of data leading to a general loss of video quality. NTSC can only deliver 720 pixels wide video or stills from video.

Digital video, or DV, on the other hand, remains digital (such as '0's and '1's ) with the data describing the colors and brightness of each video frame. On the receiving end of this data transmission, there is no translation or interpretation, just the delivery of pure data. The consistency of delivery is the crucial advantage that digital video has over analog video when it comes to working with images on a PC. As opposed to NTSC, there is no limit to resolution so images or movies as wide as 4000 pixels are easily obtainable with the digital cameras we sell for microscopy.

|  |  |  |
| --- | --- | --- |
| **Factor** | **Digital** | **Analog** |
| Signal Type | Digital Systems use discrete signals as on/off representing binary format. Off is 0, On is 1. | Analog Systems use continuous signals with varying magnitude. |
| Wave Type | Digital Systems use square waves. | Analog systems use sine waves. |
| Technology | Digital systems first transform the analog waves to limited set of numbers and then record them as digital square waves. | Analog systems records the physical waveforms as they are originally generated. |
| Transmission | Digital transmission is easy and can be made noise proof with no loss at all. | Analog systems are affected badly by noise during transmission. |
| Flexibility | Digital system hardware can be easily modulated as per the requirements. | Analog system's hardware are not flexible. |
| Bandwidth | Digital transmission needs more bandwidth to carry same information. | Analog transmission requires less bandwidth. |
| Memory | Digital data is stored in form of bits. | Analog data is stored in form of waveform signals. |
| Power requirement | Digital system needs low power as compare to its analog counterpart. | Analog systems consume more power than digital systems. |
| Best suited for | Digital systems are good for computing and digital electronics. | Analog systems are good for audio/video recordings. |
| Cost | Digital systems are costly. | Analog systems are cheap. |
| Example | Examples of digital systems include Computers, CD, and DVD. | Examples of analog systems include analog electronics, voice radio using AM frequency. |

# Display Resolution

Display resolution or screen resolution expresses how many pixels are present in a display or entire screen. A given display will have a maximum resolution that depends on its physical ability to focus light. For example, a 15-inch 640x480 monitor will display approximately 50 dots per inch.

### Overscan and underscan-

Most television display manufacturers "overscan" the pictures on their displays (CRTs and PDPs, LCDs etc.), so that the effective on-screen picture may be reduced from 720 × 576 (480) to 680 × 550 (450), for example. The size of the invisible area somewhat depends on the display device. Some HD televisions do this as well, to a similar extent.


Computer displays including projectors generally do not overscan although many models (particularly CRT displays) allow it. CRT displays tend to be underscanned in stock configurations, to compensate for the increasing distortions at the corners.

### Interlaced and progressive scan-

[Interlaced video](https://en.wikipedia.org/wiki/Interlaced_video) (also known as **interlaced scan**) is a technique for doubling the perceived [frame rate](https://en.wikipedia.org/wiki/Frame_rate) of a video display without consuming extra [bandwidth](https://en.wikipedia.org/wiki/Bandwidth_(signal_processing)). The interlaced signal contains two [fields](https://en.wikipedia.org/wiki/Field_(video)) of a video frame captured consecutively. This enhances motion perception to the viewer, and reduces [flicker](https://en.wikipedia.org/wiki/Flicker_(screen)) by taking advantage of the [phi phenomenon](https://en.wikipedia.org/wiki/Phi_phenomenon).

The [European Broadcasting Union](https://en.wikipedia.org/wiki/European_Broadcasting_Union) has argued against interlaced video in production and broadcasting. The main argument is that no matter how complex the deinterlacing algorithm may be, the artifacts in the interlaced signal cannot be completely eliminated because some information is lost between frames. Despite arguments against it, television standards organizations continue to support interlacing. It is still included in digital video transmission formats such as [DV](https://en.wikipedia.org/wiki/DV), [DVB](https://en.wikipedia.org/wiki/Digital_Video_Broadcasting), and [ATSC](https://en.wikipedia.org/wiki/ATSC). New video compression standards like [High Efficiency Video Coding](https://en.wikipedia.org/wiki/High_Efficiency_Video_Coding) are optimized for [progressive scan](https://en.wikipedia.org/wiki/Progressive_scan) video, but sometimes do support interlaced video.

[Progressive scanning](https://en.wikipedia.org/wiki/Progressive_scanning) (alternatively referred to as **noninterlaced scanning**) is a format of displaying, storing, or transmitting [moving images](https://en.wikipedia.org/wiki/Moving_image) in which all the lines of each [frame](https://en.wikipedia.org/wiki/Film_frame) are drawn in sequence. This is in contrast to [interlaced video](https://en.wikipedia.org/wiki/Interlaced_video) used in traditional [analog television](https://en.wikipedia.org/wiki/Analog_television) systems where only the odd lines, then the even lines of each frame (each image called a [video field](https://en.wikipedia.org/wiki/Video_field)) are drawn alternately, so that only half the number of actual image frames are used to produce video.



when a video is said to have a resolution of 3840×2160 pixels, it essentially means the video has a width of 3840 pixels and a height of 2160 pixels.

So right now, it must be obvious that the higher the resolution, the sharper and crisper the video image will be. Theoretically, it has more clarity because, since the number of pixels is high, there are more blocks for colors to fill in, thus giving a better image quality.

Currently, there are various types of video resolutions. There exist multiple types of video resolution rather than “One Ultimate Resolution”. When devices are manufactured, may it be mobile phones, monitors, televisions, or digital billboards, the screen resolution is predetermined. So in order to choose a video resolution, you have to understand your target devices.

For example, you might have watched movies either on television or mobile devices with the video dimension of 640 x 360, 640 x 480, or 720 x 480. Sometimes users prefer to watch clear & sharper images with brighter colors. Movies like Avatar, Avengers, Interstellar can be better viewed in high definition with the value of 1280 x 720 (720p) or 1920 x 1080.

## What is a Pixel ?


The word “pixel” refers to a picture element in an image. These pixels are the smallest unit of an image. The images comprise hundreds of thousands (and often millions) of pixels. When every pixel gets combined a resolution is formed. It will be in 3 components, known as RGB (Red, Green, Blue), or 4 components, known as CMYK (Cyan, Magenta, Yellow, blacK).

## What is the Aspect Ratio?

If you are to understand the different types of video resolutions, you need to understand what the [video aspect ratio](https://www.vdocipher.com/blog/video-aspect-ratio/) is and why it is important.

Aspect ratios, in simple words, are the ratio of horizontal pixels (width) to vertical pixels (height).

For example, if a device is known to have a predefined resolution of 1920×1080 pixels, it has an aspect ratio of 16:9.

[](https://www.vdocipher.com/blog/wp-content/uploads/2021/09/video-resolution-aspect-ratio.png)

Most videos on the internet have an aspect ratio of 16:9, as it is said to support the majority of devices, even television screens.

The reason aspect ratios are an important factor to consider is that it affects the final display and makes sure the cropping is not limited where it should not be.

If you are producing a video of aspect ratio 1:1, it can be concluded that wherever it is displayed, it is displayed as a proportional square. So knowing about the [video aspect ratio](https://www.vdocipher.com/blog/video-aspect-ratio/), in the beginning, helps you understand how the final video image will be produced and how it will be displayed on different screens.

## What is the meaning of P and I in Resolution?

‘P’ refers to Progressive video where it makes use of horizontal lines to make up the image. examples to consider 480p, 720p or 1080p. Displays both the scan lines (even & odd) simultaneously. This type of videos results in better, fast sequences providing sharpness to the video. The progressive display is used in all monitor screens.

‘I’ refer to interlaced video. This technology was introduced in the early days of television to fit a picture into the desired bandwidth. An example to consider 480i or 1080i. It displays even and odd scan lines in separate fields. Two of these even and odd scan line fields form one video frame.

## Different Types of Video Resolutions

Every new type of video resolution is clearer and crisper than its predecessor. Let’s go through the different types of video resolutions.

Sometimes, rather than saying a dimension, we refer to different resolutions by their names given based on how they appear on screens. The different types of video resolutions are:

* Standard Definition (SD)
* High Definition (HD)
* Full HD
* 2K resolution
* Ultra High Definition (UHD) or 4K
* 8K resolution

Each type has its own number of pixels and aspect ratios.

### Video Resolution Chart

|  |  |  |  |
| --- | --- | --- | --- |
| Resolution | Name | Aspect Ratio | Pixel Size |
| SD (Standard Definition) | 480p | 4:3 | 640 x 480 |
| HD (High Definition) | 720p | 16:9 | 1280 x 720 |
| Full HD (FHD) | 1080p | 16:9 | 1920 x 1080 |
| 2K video (Quad HD) | 2k or 1440 | 16:9 | 2560 x 1440 |
| 4K video or Ultra HD (UHD) | 4K or 2160p | 1:1.9 | 3840 x 2160 |
| 8K video or Full Ultra HD | 8K or 4320p | 16∶9 | 7680 x 4320 |

### Standard Definition

Standard Definition, as the name would suggest, does not have a lot of pixels, resulting in lower resolution. Two popular SD resolutions are 640×360 and 640×480. These resolutions are best for small mobile devices. The aspect ratio for standard video is 4:3

In Standard Definition, videos are of low quality, with lower bit rates and smaller file sizes. A good option to consider if you are on slow internet connection.  With the lower bit rate videos can be streamed more smoothly with less chance of buffering compared to higher quality videos.

### High Definition

High Definition or HD is a step ahead of standard definition. When it comes to HD resolutions, the video or screen is being specific about only two resolutions – 1920×1080 pixels or 1280×720 pixels. 1920×1080 resolution (1080p) refers 1920 pixels horizontally and 1080 pixels vertically. HD videos come with a fixed aspect ratio of 16:9. HD videos are best for small online content. You can read more about [SD vs HD](https://www.vdocipher.com/blog/sd-vs-hd) in this blog.

### Full HD

Full HD is the same as HD, but the resolution is strictly 1920×1080. In other words, full HD videos are strictly 1080p.

‘p’ here refers to progressive scan. It is the type of display and signal used to refresh the pixels periodically. This resolution is widely used in most smartphones currently.

### 2K Resolution

2K Resolution is also known as Quad High Definition (QHD). Quad High Definition is so much more advanced than HD or Full HD. Most commonly used in advanced smartphones and gaming monitors. It has an aspect ratio of 1:1.77 and the dimensions are 2048×1152 pixels.

### Ultra High Definition

Ultra High Definition is commonly known as 4K resolution. Generally speaking, there isn’t much difference between 2K and 4K. The only difference is, since the size is comparatively bigger, it adds more space to zoom in. There won’t be any noticeable difference unless the color grading deep inside is very different.

4K resolutions are mostly used for the theatrical releases of movies and work well on big screens.

The dimensions of UHD are 3840×2160 and the aspect ratio is 16:9. It is commonly referred to as 2160p.

### 8K Resolution

8K Resolution is very advanced, and not widely used. But the image quality is very intense and it has a lot of space for editing and zooming. If 8K resolution is chosen, it is primarily to focus on reframing and enhanced visual effects. The dimensions are 7680×4320 pixels.

## Formats of video files-

There are numerous video file formats available that can be used for videos, which provide different-different video quality. A list is given below that has some common kinds of video files.

* **.3GP:**  3GP is a compression file format created by 3GPP (3rd Generation Partnership Project), which is a basic version of MPEG-4 part 14 (MP4) format. It is used to compress audio, video, and other multimedia to save on disk space, bandwidth, and data usage. It often creates files for use with cell phones. There are different video players that can play this file format videos on your computer, smartphone, or tablet. The .3GP or .3G2 are the file extensions of the 3GP file format.
* **.MP4:**  MP4 is a file format that was introduced in 1998, which stands for MPEG-4 Part 14 and, it was agreed upon as a standard by the MPEG. It is an audio and video compression standard, commonly used to store video and audio as well as store subtitles and still images. Like the MPEG-1 and MPEG-2 standards, MPEG-4 reduces the file size as much as possible through codified methods for encoding audio and video. It provides some features, such as DRM (Digital Rights Management) support, various forms of interactivity, including features for 3D rendering with VRML.
* **.AVI:**  An AVI file is a sound and motion picture file, stands for Audio Video Interleaved that is used for video files under Microsoft Windows. The file size, 2 GB, is the maximum file size of an AVI file. AVI files have the extension .avi and need a special player to play the video files that may be require downloading or may be included with your Web browser.
* **.WebM:**  WebM provides open video compression for HTML5 videos that are based on the same video format, which uses the MKV file extension. It is a container format for audio and video data that is sponsored by Google Inc. as a WebM Project. Under a BSD license, it was put together to provide support and release WebM content that led to available in the market to users for free of cost. If any file has the WEBM file extension, it will be a WebM Video file. As the format is used on HTML5 websites for video streaming, therefore, most web browsers support WEBM files.
* **.MOV:**  MOV is a MPEG 4 video container file format introduced by Apple in 1998. It is a format of Apple's Quicktime program. An algorithm, Apple's proprietary compression, is used by MOV files, which can be opened with the help of using a video editor, compatible video program, or QuickTime.
* **.WMV:**  The WMV file extension is a video file format, which stands for Windows Media Video and is developed by Microsoft. It is a compressed video file format that supports different video codecs for streaming video over the Internet. The .WMV is the file extension of the WMV file. It contains video encoded with one of Microsoft's WMV proprietary codec and is the same as an. ASF file. Now WMV files can be played on different player software. In 1999, it was introduced as a competitor of the RealVideo format.
* **.FLV:**  An FLV encoder tool is native to the Adobe Flash player, which is commonly used to change audio and video into the FLV format. The .FLV is the file extension of the FLV file.